| **Command** | **Variant** | **Tested Command** | **Response Example** | **Notes** |
| --- | --- | --- | --- | --- |
| **CSQ** | Test | AT+CSQ=? | +CSQ: (0-31,99) | Supported — returns valid range |
|  | Read | AT+CSQ? | ERROR | Not supported in emulator (should be) |
|  | Lenient | AT+CSQ | +CSQ: 15,99 | Emulator accepts non-standard form |
| **CMGF** | Test | AT+CMGF=? | +CMGF: (0,1) | Supported |
|  | Read | AT+CMGF? | +CMGF: 1 | Returns current SMS mode (text by default) |
|  | Set | AT+CMGF=1 | OK | Sets SMS mode to text |
| **CPIN** | Test | AT+CPIN=? | OK | Not standard; accepted but no info |
|  | Read | AT+CPIN? | +CPIN: READY | Shows SIM status |
|  | Set | AT+CPIN=1 | OK | Invalid in real modem; accepted in emulator |
| **CMGS** | Test | AT+CMGS=? | OK | Returns OK, but no valid range shown |
|  | Read | AT+CMGS? | ERROR | Not supported |
|  | Set | AT+CMGS="..." | ERROR | Emulator does **not** support actual SMS sending |
| **CMEE** | Test | AT+CMEE=? | ERROR | Not supported in emulator |
|  | Read | AT+CMEE? | ERROR | Not supported |
|  | Set | AT+CMEE=2 | ERROR | Not supported |

| **Syntax Type** | **Commands Supported in Emulator** |
| --- | --- |
| Test | AT+CSQ=?, AT+CMGF=?, AT+CPIN=?, AT+CMGS=? |
| Read | AT+CMGF?, AT+CPIN? |
| Set | AT+CMGF=1, AT+CPIN=1 (invalid, but accepted) |