| **AT Command** | **Emulator Response** | **Manual Interpretation** |
| --- | --- | --- |
| AT+CMEE=2 | ERROR | Emulator doesn't support AT+CMEE, so verbose error mode can't be enabled. |
| AT+XYZ | ERROR | Unknown/unsupported command — not implemented in the emulator. |
| AT+CSQ=1 | ERROR | AT+CSQ does not accept parameters; invalid syntax. |
| AT+CMGS=1 | ERROR | SMS send command not correctly formatted; message content expected after CMGS. |
| AT+CPIN=1 | ERROR | Invalid SIM PIN format; CPIN expects a PIN string (e.g., AT+CPIN="1234"). |
| AT+CREG=abc | ERROR | Invalid input for network registration query; accepts only ? or numeric values. |
| AT+COPS="Jio" | ERROR | Wrong format; COPS command expects numeric mode selection, not just operator name. |
| AT+CMEE=? | ERROR | Emulator does not support test mode query for CMEE. |